Event Log Interface (ELI) High Level Requirements - Singapore
Phase 1: Process Requirements:
· Create Configuration files:
· Complete and roles have been assigned to update and maintain them. 
· Plan in place to ensure consistency between config files at CMs and Milford Production. 
· Identify End Users: 
· Roles assigned to personnel who will use the ELI to input data. 
Phase 2: Hardware Requirements:
· Identify Server (can be different per site):
· Used to store the configuration files for the ELI.
· Accessible by Contract Manufacturer, WPPL, and Milford Operations Engineering. 
· Identify Host Computers (as many as needed for the number of end users at a site):
· Windows 7 (preferred) or later.
· Not a currently used computer for a tester. Can be an end users personal computer. 
· Login credentials to access to sigmaprod.corp.waters.com/sigma (on network).
· Login credentials to access to server (on network). Configuration files are read by ELI from the server. 
Phase 3: ELI Software Requirements:
· Software Updates
· Minor updates required to accommodate new sites.
Phase 4: Installation Requirements:
· SigmaProbe and SigmaProbeAPI
· Must be installed on all host computers to communicate with SigmaSure.
· Must be configured on all host computers.
· Event Log Interface Software
· Must be installed on all host computers.
Phase 5: Process Requirements:
· Release Event Log Template 730001377 to CMs: 
· Template updated at contract manufacturers and operators trained. 
· Guidance documents are provided to operators on the floor.
· Train End Users of ELI, templates, and configuration files. 
Phase 6: Validation Requirements:
· CSV: Software Tool Validation Procedure
· Software Validation Assessment Form needed to asses changes and new installations.
· Installation Qualification likely required on host computers. 
