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INPUT VOLTAGE: 230/240VAC


FREQUENCY: 50/60Hz


CURRENT: 2A 		





OUTPUT VOLTAGE: 48V DC


CURRENT: 5A max





5A Anti-surge





5A Anti-surge





5A Anti-surge





TB594 APGC BAKING TEST BOX








COVER TO BE REMOVED BY WATERS TRAINED PERSONNEL ONLY!








