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This procedure documents how to install and configure a Windows NT Workstation for use in the Universal Front End Tester. This procedure assumes the appropriate add in boards have already been installed.

Start by performing a fresh Windows NT installation, see Windows NT Installation Notes.doc.

1. Login as administrator

2. Insert the System Installation Disk into the CDROM drive.

3. Using either the Program Manager (My Computer) or Windows NT Explorer open and view the contents of the CD.

4. Install WinZip

a. Open the WinZip folder, and double click file winzip80.exe

b. In the WinZip 8.0 Setup window click the Setup button
c. Click OK to install WinZip to the default directory C:\Program Files\WinZip

d. Follow the setup instructions and use default options when asked.

e. It is not necessary to restart the PC at this time.

5. Install Adobe Acrobat Reader

a. Open the Adobe folder, and double click file ar505enu.exe

b. Follow the setup instructions and use default options when asked.

c. It is not necessary to restart the PC at this time.

6. Install Printer Drivers

a. Open the Print Drivers folder, and double click file SETUP.EXE

b. From the Setup window click on Install HP Deskjet 610C Series Printer Software

c. Follow setup instructions using default options when asked.

d. Click on Cancel when asked to Install Bonus Software

e. Click Yes to confirm Cancel.

f. It is not necessary to restart the PC at this time.

7. Install Video Drivers

a. Open the Video Drivers folder, and double click file ATISETUP.EXE

b. From the Setup Window select ATI Easy Install
c. Follow setup instructions using default options when asked.

d. Select to restart the computer when prompted to do so.

e. Login as the administrator

f. Configure the Display Settings as follows:

g. Color Palette:

65536 colors

h. Desktop Area:

1024 x 768 pixels

i. Font size:

small fonts

j. Refresh frequency:
60 Hertz

k. Click to apply settings. No need to test or restart

8. Install GPIB drivers

a. Open the GPIB Drivers folder, and double click file ni488216.exe

b. Click on the Setup button

c. Follow setup instructions using the following options:

i. Do not register online

ii. Use the default Destination Directory

iii. Do not install Development files and Samples (uncheck option when in the Select Components window

d. Allow system to restart when finished installing

e. Login as administrator when system restarts

f. At this point the NI-488 Getting Started Wizard will automatically start and aid the user in configuring the GPIB hardware. Follow the instructions carefully. Select board type PCI-GPIB when instructed to do so.

g. It is not necessary to restart the PC at this time.

9. Install DAQ Drivers

a. Open the DAQ Drivers folder, and double click file SETUP.EXE

b. After the installer initializes it may request that you restart the system, do so. The installer will restart automatically after the PC restarts and you Login as administrator.

c. Click Next>> to continue.

d. Accept the License agreement

e. Review the Feature Tree. The only feature we want to install is DAQ Drivers. If the NI-OPC Server feature is setup to install:

iv. Click on the feature

v. Choose option: Do Not Install this Feature

f. Continue to complete installation

g. Reboot when prompted to do so

h. Login as administrator

i. Setup will automatically restart with the option to Configure Measurement and Automation System enabled. Click Finish to complete the configuration

j. The Measurement and Automation Explorer is started. The User Preferences window is displayed. Click the Every time I launch MAX option and uncheck the Show this dialog every time I launch MAX option. Click OK
k. MAX shows detailed instruction in the left window. Use them to configure Devices and Interfaces:

vi. Select Devices and Interfaces
vii. Highlight PCI-6025E
viii. Right click and select Properties
l. In the Configure Devices window select the AI tab

m. Change Mode to Nonreferenced Single Ended

n. Select the Apply button at the bottom of the window

o. Select OK at the bottom of the window

p. Close MAX.

10. Install PreAmp Tester application software

a. Open the PreAmp Tester folder.

b. Double click the Setup file.

c. Click Finish to complete the installation

d. Close all windows and restart the computer.

11. Test software and driver installation

a. Start the test system: Start>>Programs>>Preamp Tester>>PreAmp Tester
b. When the tester application initializes errors will pop up if the drivers are not configured properly

12. Install the Tweak UI

a. Open the TweakUI folder, and double click file tweakui.exe

b. In the WinZip Self-Extractor pop-up verify the destination directory is C:\temp. Click Unzip. Then close the WinZip Self-Extractor window

c. Using either the Program Manager or NT Explorer navigate to directory C:\temp
d. Locate and highlight the file tweakui.inf
e. Right click and select Install from the pull down menu.

13. See document Configure Windows NT.doc to setup users, security, and startup options.

