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This document details the process of installing Windows NT on the Universal Front End Tester. It may be used if an existing system should crash or if the system needs to be duplicated.

1. Reboot PC with Windows NT Setup Disk 1 in the floppy disk drive A:

2. Replace Setup Disk1 with Setup Disk2 when prompted to do so.

3. Press ENTER to setup Windows NT when prompted to do so.

4. Press ENTER to auto-detect mass storage devices.

5. Replace Setup Disk2 with Setup Disk3 when prompted to do so.

6. When Setup detects the CDROM drive press ENTER to continue.

7. Press ENTER to confirm setup has detected a hard disk with more than 1024 cylinders.

8. Insert Windows NT 4.0 Workstation CD into the CDROM drive and press ENTER to continue.

9. Page down to bottom of License Agreement and press F8 to accept.

10. Press N to install a fresh copy of Windows NT.

11. Press ENTER to confirm the detected hardware configuration.

12. If bringing up a unformatted hard drive:

a. Create a partition from unpartitioned space

b. Make the partition 4096 megabytes. This partition should automatically be assigned drive letter C

c. You may then create another partition from unpartitioned space and the size may be the remaining space available

13. Highlight partition C: and press ENTER to install NT on this partition.

14. Format using NTFS file system.

15. Confirm that all data will be lost, press F.

16. When finished formatting, Press ENTER to confirm the default location for NT.

17. Press ESC to skip an exhaustive examination of the disk drive.

18. When finished copying files remove Setup Disk3 and the Windows NT CD. Press ENTER to restart the PC.

19. Insert the Windows NT CD when prompted to do so.

20. Press ENTER whenever a window displays the Next>> button.

21. Select Typical Installation, and press ENTER.

22. Enter:

a. Name:
Test Engineering

b. Organization:
Waters Corporation

23. Enter Product ID, located on the Certificate of Authenticity

24. Enter Computer Name:
PreAmp Tester

25. Enter Administrator account Password:
administrator

26. Do not create an Emergency Repair Disk.

27. Select Install the Most Common Components

28. Select Not to Connect to Network at this Time.

29. Finish Setup:


a. Enter the time zone

b. Verify and change if necessary the date and time

c. Acknowledge video settings

30. Remove Windows NT CD and restart the PC

31. Login to the Administrators account. Remember the password?

32. Insert Windows NT Workstation Service Pack 6 CD into the CDROM drive.

33. The Service Pack installer will auto-run.

34. Select Install Service Pack 6

35. Select Install Service Pack 6 for Intel-Based Systems

36. Confirm Open File “update.exe”

37. Accept License Agreement and install.

38. Restart the PC and login as the Administrator.

39. See document Install and Configure Test System.doc to install the required software components and configure the system to run in the Universal Front End Test System.

