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ACQUITY UPLC H-Class PLUS 
Feature Highlights
1. Automatic and continuous compressibility compensation – Users are not required to enter compressibility values for mobile phase on Instrument Method. Please check the attached system specification and instrument method print screen below. (add a print screen of QSM instrument method tab below)
2. Automated purge – System priming/purging is solely controlled through Empower 3. Users are not required to manually switch valve (on pumps) during priming/ purging.
3. Active seal wash –This system has an additional solvent line for seal wash that actively flush the rear of the high pressure seals and the plungers. This design avoids cross-contamination that may be caused by close-loop seal wash on other conventional LC systems.
4. Active needle wash – This system has an additional solvent line for needle wash that actively washes the exterior of the needle. This design significantly improve the carryover issue that may occur on LC that has passive needle wash.


Empower 3
Feature Highlights
1. Seamless integration of PDA and mass data – Data acquired using PDA and ACQUITY QDa Mass Detector/ SDQ2 (in tandem) can be processed concurrently for calibration, quantitation, purity and library matching. Users are not required to process the PDA and MS data separately.
2. Custom reporting – Empower 3 provides high flexibility for users to customize reporting format and template.
3. Custom field – Extra fields (can be user-entry information or calculation) can be created within Empower 3. This feature allows workflow automation and reduces human error.
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