Lambda Power Supply Configuration
The Rear Panel Dip switch settings:

Sw1
down

Sw2
down

Sw3
down

Sw4
down

Sw5
down

Sw6
UP

RS485 interface  ( For PS2 - PS6 )  ( For PS1 Sw6 is down )
Sw7
down

Sw8
down

Sw9
UP

Rear Panel Enable/Disable control is Active (see DB25 connector)

Five pin green phoenix connector:
Pin 1
S+
wired to VPC interface

Pin 2

Pin 3

Pin 4

Pin 5
S-
wired to VPC interface

DB25 connector:

Pin 1
Enable/Disable control signal wired to VPC interface micro-switches
Short = PS Enabled

Pin 14
Enable/Disable control signal wired to VPC interface micro-switches
Open = PS Disabled

(all other pins open)

