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1.0  
OBJECTIVE

This document provides test procedures for W1210000478 PCBA with TE82988-3 test station.
2.0
SCOPE

This procedure is applicable to all well trained test operators or whoever using TE82988-3 test station when testing a PCBA.
3.0
RESPONSIBILITY


Test Engineer is responsible for any procedure changes
4.0
PROCESS FLOW CHART


N.A
5.0 PROCEDURES
5.1 Test Procedures

5.1.1 Before testing, ensure that the entire tester instrument equipped is all in power on state together with the tester PC.

5.1.2 Always wear the wrist trap before testing or doing a board handling.

5.1.3 Check what PCBA number for testing and match with the correct FCT test fixture and engage to the tester.
5.1.4 Click to open the icon highlighted shown below (Fig 1) to launch the Operator Interface 
(Fig 2).
Fig 1
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Fig 2
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5.1.5 Click the “Test UUT“ button of the operator interface software as shown in Fig 2. 
5.1.6 After which click the “Select Board” for test software selection as shown below.
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5.1.7 After click the Select Board button, a software window prompt for the board number selection. Select the “CM-A Personality Card – 210000478“as shown below.
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5.1.8 After selecting the desired software, click the OK button as shown below.
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5.1.9 After “OK“ button is click it means the test software already selected and the message box for board selection automatically disappear.
5.1.10 Click or press the “Test UUT’s“button shown below to completely load the test software.
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5.1.11 Wait for a while until the test software is fully loaded or initialize. A software box for the Serial Number entry prompt once the test software completely loads as shown below.
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5.1.12 Place the UUT or board for testing on the bed of test fixture and connect the high-density cable for the CPU intended to the UUT.
5.1.13 Scan the Serial Number of the board for testing. Below is the example of how to scan the board serial number correctly to avoid scanning the wrong number.
[image: image8.png]



5.1.14 After scanning the correct serial number, click the “OK” button or hit the Enter key of the keyboard.
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5.1.15 The Vacuum will turn on to pull the UUT down onto the bed of nails. The system will verify proper seating of the top plate on the fixture and then power will be applied.   The testing will now begin.  

5.1.16 Upon completion of the test, the vacuum will release and the results (pass, fail) will be displayed. If the entire test passing a pass result window as shown below will prompt. Otherwise it show fail for fail board.
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5.1.17 Failures will be displayed in an open window on the monitor. 

5.1.18 Those UUT failed; tag them with reject tag with the failure description.
5.1.19 Those UUT passed, stamp it with FCT stamp then remove from the test fixture. Make sure to put in a separate bin/box to avoid mixing from other untested or fail board.
5.1.20 Test the remaining board following the test procedure from the beginning.
6.0 KEYWORD, ABBREVIATIONS and DEFINITIONS

6.1 Keyword, Abbreviation and Definition is stored in Keyword, Abbreviation and Definition Masterlist which is available directly in GES Singapore QM, SOP, WI and other document and records Lotus Notes Database (Filename: DocControl2\NewSOP.nsf)
N.A
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