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Sap zip file
Output File Information:

1. Part number: 361000408
2. Description:  PRODUCTION MASTER, 361000408, U1
3. Development Programming File Name (.jic): 361000408_RevC_01112012.jic
4. JIC  File Checksum:  0x027935D8
5. Development Programming File Name (.sof): 361000408_RevC_01112012.sof
6. SOF File Checksum: 0x000D69EC   
7. FPGA Version Number:  5
Tools:

Quartus II Software Version 9.0 Build 132 2/25/2009 SJ Full Version 
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Source Code Retrieval Procedure:

Load from SAP
Design Summary
1. The BSM Head Cooler PCB does not have a CPU2000 so FPGA image is loaded from serial Flash on power-up.

2. 361000408 Design is for Altera Cyclone 3 FPGA 332000789, however program resides in non volatile Serial Flash 332000790.

3. To program Flash device the FPGA JTAG interface can be used with a .JIC file.  The Altera FPGA has internal hardware that allows the JTAG interface to load program into serial Flash.

4. The Serial Flash can also be programmed by in-circuit tester using a .hexout file.  The .hexout file should be generated from the .sof file defined by the 361000408 design

Design Modification Procedure (if necessary):
5. Open Quartus II Software Version 9.0. with project files.

6.  Edit design
7. Update Rev and recompile.
Recompile Procedure:
1. Open Quartus II Software Version 9.0.

2. Open Project by link (FILE => OPEN PROJECT) then find project “TOP.qpf” in design folder.
3. Next start compilation by path (PROCESSING => START COMPILATION)
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