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1.0 OBJECTIVE


To define a test procedure for GR2286 In Circuit Tester.
2.0
SCOPE

This procedure is applicable to all test personnel.


3.0
RESPONSIBILITY

Test Engineer is responsible for any test procedures changes.
4.0
PROCESS FLOW CHART


N.A.
5.0 PROCEDURE

5.1 Initial Setup
5.1.1 Check and ensure that the compress air and vacuum is ON.
5.1.2 Power on the tester thru the switch located at the back of the tester.
5.1.3 Power on the tester test head thru the panel switch highlighted with red as shown below.
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5.1.4 Turn on the PC power and the printer.

5.1.5 After a while a window prompting for Log-In information. No password required instead select or click “Administrator” to continue.

5.1.6 Check the PCBA model number for testing and confirm the test fixture number in the PCBA Test Fixture List “ENG-081“. Refer to the attachment in section 9.0.
5.1.7 Place the test fixture onto the bed of the tester by aligning the vacuum well hole of the fixture to the tester as shown below.
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5.1.8 Lock the test fixture into the tester test head by pushing down the fixture vacuum lever in the “LOWER“ position highlighted with red as shown below.
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5.2 Test Software Loading and Board Testing
5.2.1 On the desktop, double click below ICON to launch the software.
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5.2.2 Test software directory window menu will prompt for test software selection. Select ‘users’ as shown below.
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5.2.3 After selecting “users”, select “gr228x” as shown below.
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5.2.4 After which, select “boards” as shown below.
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5.2.5 Once test program directory is locate or after executing steps 5.2.1 to 5.2.4, confirm what PCBA number for testing and select the test software accordingly in the directory as shown below. Test software of individual PCBA is separated and determined by folder with the PCBA number model. Refer to “ICT Master List“ form number ENG-053 for the test software complete list.
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5.2.6 After selecting the correct folder for test software path, click “ OK “ and the user interface window as shown below will prompt.
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5.2.7 Press or click “ RUN “ button of the user interface window in step 5.2.6 to proceed with the Runtime System window as shown below.
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5.2.8 Scan the serial number of board for testing to the space provided then place it in the bed of nail test fixture. Clamped the board then click the “Start” button in the runtime system window shown in 5.2.7. Alternatively, press the “LEFT“button of the manual controller as shown below.
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5.2.9 Testing will take a while to complete the test. Either Pass or Fail test result will show after testing.
5.2.10 If board passes all the test, the result will show pass as shown below.
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5.2.11 Otherwise, If one of the test fail the test result is fail as shown below.
[image: image13.emf]
5.2.12 If board passed the test, stamp it with ICT stamping before removing from the test fixture then put in the pass box or bin.
5.2.13 Continue do the testing with the other board following the test procedure from step 5.2.8 to 5.2.12
5.3 Board Segregation
Ensure the boards are clearly segregated using the tags as shown below. 

Each carton or tray must not house more than 1 category of board.

Awaiting ICT      Boards awaiting to be tested

Failed ICT         Boards fail at ICT

Passes ICT       Boards Passed at ICT
6.0 
KEYWORD, ABBREVIATIONS and DEFINITIONS
6.1 Keyword, Abbreviation and Definition is stored in Keyword, Abbreviation and Definition Masterlist which is available directly in GES Singapore QM, SOP, WI and other document and records Lotus Notes Database (Filename: DocControl2\NewSOP.nsf)
N.A
7.0 
REFERENCES
7.1  ASSOCIATED EXTERNAL DOCUMENTS
	Document 
	Reference description

	N.A
	N.A


7.2   ASSOCIATED INTERNAL DOCUMENTS

	Document type
	Document number
	Document title

	Form
	ENG-081
	PCBA Test Fixture List


8.0
RECORDS CONTROL

	Record
	Retention Period
	Location
	Responsible

	N.A
	N.A
	N.A
	N.A


9.0 
ATTACHMENT/APPENDICES
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