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Equipment Required

	Quantity
	Part Number
	Description

	None
	
	

	
	
	


Disposables Required

	Quantity
	Part Number
	Description

	None
	
	

	
	
	


reference documentation

	Document Number
	Description

	735003678
	Generic PC Maintenance Procedure

	735002229
	CM-A Test Procedure

	735002236
	Test procedure, Aux CM-A


1. Conector Inspection
1.1. Inspect all UUT interface connectors replace any that are worn or damaged.

2. PC Maintenance

2.1. Perform PM or TE83026 PC per 735003678, Generic PC Maintenance Procedure.

3. Waters’ instrument maintenance

3.1. Verify that system CMA and CM AUX have valid PM’s if not send units for PM.
4. Maintenance Complete

4.1. Fill out PM slip and place PM stickers on tester(s).
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