Waters Corporation

Calibration / maintenance Procedure
COMPANY CONFIDENTIAL

	DOCUMENT NAME:
	15kPSI Actuator tester Maintenance Procedure

	DOCUMENT TYPE:
	
 FORMCHECKBOX 
  Calibration

 FORMCHECKBOX 
  Maintenance

	TEST EQUIPMENT NAME:
	15kPSI ActuatorTester

	TEST EQUIPMENT NUMBER:
	TE82800

	DOCUMENT NUMBER:
	735002844


	AUTHOR(S):
	Matt Brule
	DATE:
	January 24, 2013

	REVISED BY:
	MATT BRULE
	DATE:
	January 29, 2013

	REVISION:
	B


	VALID IF CURRENT EFFECTIVE REVISION AND STAMPED IN RED BY DOCUMENT CONTROL OR WITH SAP-GENERATED TIME & DATE STAMP.


Equipment Required

	Quantity
	Part Number
	Description

	2
	
	5/16” wrench

	1
	
	¼” box wrench

	
	
	

	
	
	

	
	
	

	
	
	


Disposables Required

	Quantity
	Part Number
	Description

	
	
	

	
	
	


1. VISUAL INSPECTION / CLEANING
1. Visually inspect all UUT interface fittings, replace if worn.
1. Inspect all UUT interface Cables and connectors, replace as necessary.
2. Verification
2. Test a known good actuator per test procedure 735001029.
3. End of preventative maintanence

3. Fill out PREVENTATIVE MAINTANENCE sticker and place on Test System.

THIS DOCUMENT AND ITS CONTENTS ARE EXCLUSIVE PROPERTY OF WATERS CORPORATION, MILFORD MASSACHUSETTS.  THIS DOCUMENT MAY NOT BE REPRODUCED IN ANY FORM WHATSOEVER, WITHOUT PRIOR WRITTEN PERMISSION FROM WATERS CORP.

Document No.: 735002844/Rev. B
Page 1 of 1
Form Revision 1.0 - March 22, 2012

Document No.:      /Rev. Error! Reference source not found.
Page 2 of 4
Company Confidential


