Rework the following components on only the circuit that fails its test!

Preheater 1 (top) 
CHC1 Preheater 1
1. Replace R16 with a new 5.36K resistor 344000766.

1. Replace R157 with a new 27.4K resistor 344000769.

2. RETEST 

Preheater 2 (bot) 
CHC1 Preheater 2
1. Replace R15 with a new 5.36K resistor 344000766.

2. Replace R164 with a new 27.4K resistor 344000769.

3. RETEST 

Heater cooler 1 (top)  
CHC1 Heater-Cooler 1
1. Replace R18 with a new 5.36K resistor 344000766.

3. Replace R22 with a new 27.4K resistor 344000769.

4. RETEST 

Heater cooler 2 (bot)
CHC1 Heater-Cooler 2
2. Replace R17 with a new 5.36K resistor 344000766.

3. Replace R158 with a new 27.4K resistor 344000769.

4. RETEST 

