IQ-04 Test Software and Instrument Firmware Version
Screenshot of Test Software showing Version 0.0
[bookmark: _GoBack][image: ]

Screenshot of BSM interface showing Micro BSM Firmware Version 1.50.221.
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File Edit Operate Tools Window Help
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“Write Command in Input Buffer then click Enter key™"

initialize Pump: sysiit
Prime Pump: runprime
Show Alarms: printAlarm

Edt - car the dta

St -setthedata

[ Component (enabled) - commands that manipulate components.
idle - idlethe component

startupDiag - run the startup diagnostics

validate - validate the component conifg

hookup - hookup the component
feset - Reset the component

dump - Dump a component

listtype - List component names by type.
it - Listallthe component names

cmdmon (enabled) - Command monitor built-in commands.
editKeys - List the command line edit keys

fime - emits seconds since power on

version - Report the application version

emdmon - Manage the cmdmon attributes
package - Manage the installed packages

help - Print this table

unalias - Remove a command alias

alias - Create a command alias

repeat - Repeat the following command

cat - Runs each of its arguments as a command
sieep - Delay execution by seconds.

spawn - spawn the following command as a threadl
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