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Test Script #     
	IQ-01
	IQ Test Name:     
	Associated Documentation Verification

	[bookmark: _Hlk14180957]Equipment #     
	TE82526-4
	[bookmark: _Hlk14181388]Equipment Name:     
	Pump Tray Tester

	Installation Site:     
	Flextronics Contract Manufacturing Site in Singapore

	Purpose: 
To verify that supporting documentation is available prior to the completion of qualification.
Test Execution:
· List all applicable documents (Preventive Maintenance, Calibration, Operating Procedures, Test Specification Procedures, Manufacturing Procedures, etc.) under the Document type header, then complete the table below. Rows may be added/removed as needed. 
· All applicable documents must have a status of Ready, Pre-Rel-Prod, or Release General in SAP. If applicable documents are unavailable in SAP state why in the comments section. 
Objective Evidence:
Completed IQ-01 Test Script Data Sheet 
SAP screenshots of below available document(s) 

	Document Type
	Title, Doc. #, Version/Revision #
	Status in SAP
	Initial & Date

	TSP
	TEST SPECIFICATION AND PROCEDURE, ALLIANCE PUMPTRAY, Rev 09
	Release
General
	HZ 27Mar20

	Comments: N/A












[bookmark: _GoBack]

	Overall Test Conclusion
		
	Document No.: ______________________

	
	Iteration No.: ________

	
	Attachment: _______  Page: ___ of ___




	 Pass			 Fail
	



	


Test Script #
	IQ -02
	IQ Test Name:
	Site Verification

	Equipment #
	TE82526-4
	Equipment Name:
	Pump Tray Tester
	Installation Site:
	Flextronics Contract Manufacturing Site in Singapore
	Purpose: 
To verify the location in which the test equipment is to be installed is suitable for use.
Test Execution:
· List additional applicable parameters in the Parameters column. Rows may be added as needed.
· Using the applicable equipment documentation, define the specification(s) in the Acceptance Criteria column. 
· Verify and/or measure the applicable parameters and complete the Table below. Do not delete any of the listed defined parameters. Enter N/A for any parameter or cell that is not used or applicable. The reason for why the parameter is not used or applicable shall be explained within the corresponding Installation Qualification Report.
Objective Evidence:
Completed IQ-02 Test Script Data Sheet
Photo(s) of the work area, as applicable
The source of each Acceptance Criterion shall be referenced in the IQR if stored in SAP. If not in SAP objective evidence specifying the Acceptance Criterion shall be provided in or as an attachment to the IQR.
Copies of calibration certificates for measurement tools, if applicable

	Parameters
	Acceptance Criteria
	As Found
	Pass/Fail
	Initial & Date

	Ambient Temperature
	18 ºC to 28 ºC
	21 ºC - 22 ºC
	Pass
	HZ 27Mar2020

	Relative Humidity
	10 % to 80 %, 
Non-Condensing
	54 % to 55%
	Pass
	HZ 27Mar2020

	Electrical Supply
	100 VAC to 240 VAC, 
50 Hz/60 Hz ±5%
	239.7 VAC
50 HZ
	Pass
	HZ 27Mar2020

	Electrical Outlets
	Minimum of 4 
dedicated outlets
	4
	Pass
	HZ 27Mar2020

	Network Available
	Minimum of 1
dedicated network
	1
	Pass
	HZ 27Mar2020

	Workspace
	The system has sufficient room 
for the test station, UUT and service
	Pass
	HZ 27Mar2020

	Test Station Bench
	The Test Station Bench is large and 
strong enough to support the station
	Pass
	HZ 27Mar2020

	Comments:
• Ambient temperature/humidity measured using a Temperature/Humidity Meter, Control Number EQID: 0418
• Electrical supply measured using a Multimeter, Control Number EQID: 0245

Note: If the electrical supply range or tolerance is not specified for voltage and/or frequency, a tolerance of ±5% may be used in accordance with ANSI C84.1 – Voltage Tolerance Standard.


	Overall Test Conclusion
		
	Document No.: ______________________

	
	Iteration No.: ________

	
	Attachment: _______  Page: ___ of ___




	 Pass			 Fail
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Test Script #
	IQ-03
	IQ Test Name:
	Instrumentation Calibration Verification

	Equipment #
	TE82526-4	Equipment Name:
	Pump Tray Tester
	Installation Site:
	Flextronics Contract Manufacturing Site in Singapore
	Purpose:
To verify that all critical instruments are in the calibration database and that a calibration and/or a preventive maintenance has been performed, as appropriate.
Test Execution:
List all critical instruments/components and/or sub-systems that require calibration and/or preventive maintenance in the Description column. Rows may be added as needed. 
Verify that all listed critical instruments/components have had a preventive maintenance and/or calibration performed in accordance with the PM and/or Calibration procedure(s) or by an outside source, and are listed within the associated calibration database, then complete the table below. 
Objective Evidence:
Completed IQ-03 Test Script Data Sheet
Copies of calibration and/or maintenance certificates
Screen captures from the associated Calibration database

	Description
	Asset #
	Cal/PM Dates
	Initial & Date

	Electronics Weigh Balance
	12200404
	Last Cal/PM: 13-Jan-2020
Cal/PM Due: 13-Feb-2020
	HZ 27 Mar 2020

	Comments:

· Electronics Weigh Balance is the only equipment that require calibration






	Overall Test Conclusion
		
	Document No.: ______________________

	
	Iteration No.: ________

	
	Attachment: _______  Page: ___ of ___




	 Pass			 Fail
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Test Script #
	IQ-04
	IQ Test Name:
	Test Software and Instrument Firmware Version

	Equipment #
	TE82526-4	Equipment Name:
	Pump Tray Tester
	Installation Site:
	Flextronics Contract Manufacturing Site in Singapore
	Purpose:
To verify that the installed software/firmware is correct per the applicable design and/or operational document(s).
Test Execution: 
List all relevant Equipment software and/or instrument firmware in the Description column. Specify the associated part number for the instrument firmware, if applicable. Rows may be added/removed as needed. 
List the associated required equipment software and/or critical instrument/internet connection sharing firmware version(s), as defined in the applicable design/operational document(s), in the Acceptance Criteria column.
Verify that the software version displayed on the Operator Interface of the program and/or the firmware loaded on the instruments/PC match the acceptance criteria identically, if applicable, then complete the table below.
Objective Evidence:
Completed IQ-04 Test Script Data Sheet
Identify and/or provide a screen capture/print out/copy of the applicable design/operational document that defines the required software/firmware version(s) within or as an attachment to the associated Installation Qualification Report.
Screen capture and/or test record displaying/indicating the software and/or firmware version(s), as applicable

	Description
	Acceptance Criteria
	As Found
	Pass/Fail
	Initial & Date

	TE82526 Test Software
	Version:  1.0
	  Version: 1.0
	Pass
	HZ 27 Mar 2020

	Comments:

· This test station does not download firmware.
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	 Pass			 Fail
	





	


Test Script #
	IQ-05
	IQ Test Name:
	General Safety and Alarms

	Equipment #
	TE82526-4	Equipment Name:
	Pump Tray Tester
	Installation Site:
	Flextronics Contract Manufacturing Site in Singapore
	Purpose:
To verify that the equipment can operate in a safe manner, within its designated location.
Test Execution:
List any additional safety related conditions or alarms in the Safety Inspection column, such as: guarding, interlocks, thermal or mechanical safety, chemical, secured gas tanks, restart or power loss, emergency stop, environmental exhaust, electrical safety, noise, safety labels, etc. Rows may be added as needed. EH&S shall be consulted as necessary.
List the associated safety requirement(s)/specification(s) in the Acceptance Criteria column. 
Perform an inspection/test of the equipment to assess its safety related conditions, then complete the table below.
Objective Evidence:
Completed IQ-05 Test Script Data Sheet
Photo(s) of the secured glass bottles, tanks, etc., if applicable
The source of any applicable Acceptance Criterion shall be summarized in the IQR if stored in SAP. If the source is not stored in SAP, at a minimum the page specifying the applicable Acceptance Criterion shall be provided as an attachment.

	Safety Inspection
	Acceptance Criteria
	Pass/Fail
	Initial & Date

	Mechanical Safety/
Pinch Points/Sharp Edges
	None Found (or mitigated appropriately)
	Pass
	HZ 27 Mar 20

	Glass Bottles
	Secure
	Pass
	HZ 27 Mar 20

	Waste Tanks
	Secure and located below the system
	Pass
	HZ 27 Mar 20

	Emergency Stop
	System ceases operation upon 
depressing the Emergency Stop button
	N/A
	HZ 27 Mar 20

	Guarding
	Shielding in place to prevent 
hazard during operation
	Pass
	HZ 27 Mar 20

	Comments:  N/A
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	 Pass			 Fail
	

	
	

	



Test Script #
	IQ-06
	IQ Test Name:
	Functional Verification

	Equipment #
	TE82526-4	Equipment Name:
	Pump Tray Tester
	Installation Site:
	Flextronics Contract Manufacturing Site in Singapore
	Purpose:
To verify that the system operates as expected.
Test Execution:
Select the UUT(s) or tests to be performed as defined within the Installation Qualification Section of 730001835.
List the Part Number and Serial Number, if applicable, in the UUT Part Number/Serial Number column.
Define the appropriate Acceptance Criteria within the Acceptance Criteria column.
Perform a test of the UUT(s), verify the Acceptance Criteria, then complete the table below. If an associated Test Record is being used as objective evidence the Header/Footer information should be verified for accuracy.
Objective Evidence:
Completed IQ-06 Test Script Data Sheet
Copy of the Test Record(s) for the UUT(s), as applicable
The UUT(s) selected for this Test Script and the reasoning for why it/they were selected shall be summarized within the associated Installation Qualification Report.
If this Acceptance Criteria is other than “All required CTQ Specification measurements result in a Pass” then it shall be summarized within the associated VAF, Process Validation Plan, and/or Installation Qualification Report.  
For systems that download firmware to product the BOM showing the firmware requirement shall be provided within the IQR.

	UUT Part Number/Serial Number
	Acceptance Criteria
	Pass/Fail
	Initial & Date

	  Part Number:    289000526
  Serial Number:  13LOHO42
	All required CTQ Specification measurements result in a Pass
	Pass
	HZ 27 Mar 2020

	Comments:  N/A
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