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	ITEM
	QTY
	PART NUMBER
	DESCRIPTION

	1
	1
	332000790
	IC, PLD, UNPROGRAMMED,M25P32-VMF6TP

	2
	(REF)
	361000408
	PRODUCTION MASTER,  BSM/SFC

	3
	(REF)
	361000408
	RECREATE PROCEDURE,    BSM/SFC

	
	
	
	



Reference Designation


PLD Part Number


Version 





WATERS 2012 (


U1


361000408


Rev. C





NOTES:


PLD to be programmed via the in-circuit test


     fixture





PLD to be labeled as presented below using PERMANENT LABEL OR EPOXY INK.





Unless Otherwise


Specified





All dimensions are in inches.


Dimensions in brackets [     ]


are in metric.


Remove all burrs and sharp


edges.





Tolerances:


Decimals





          .xx      = ( .01


        .xxx      = ( .005


       Angles  = ( 1(





Surface Roughness    63








Do not scale print.





For Dimensioning and


Tolerancing


Use Ansi Y14.5M 1982
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THIRD ANGLE PROJECTION





Next Assy:








This drawing and all information


hereon is the property of


Waters Corporation.  Any copying,


reproduction or unauthorized


use is forbidden without


written consent.














